**Risk Assessment – Last One Standing & Duck And Run**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Hazard Area** | **Risk** | **Existing Controls** | **Likelihood****1 - 5** | **Severity****1 - 5** | **Risk Score****L x S** | **Further Action to take** |
| Last one & Duck and run | Over enthusiastic participants | Responsible person supervising at all times. Rocking from side to side is NOTPERMITTED UNDER ANY CIRCUMSTANCES. | 2 | 1 | 1 | In the event of large numbers of participants trained operators will besupplied with the inflatable to aid with large numbers. |
|  |  |  |  |  |  |  |
| Last one & Duck and run | Larger participants colliding withsmaller participants | Responsible person supervising at all times. | 1 | 1 | 1 | Participants put into groups of similar size. |
| Last one & Duck and run | Larger participants colliding withsmaller participants | Responsible person supervising at all times. | 1 | 1 | 1 | Participants put in two groups of similar size. |
| Last one & Duck and run | Adverse weather conditions. | The item will be switched off in heavy rain and is not permitted to run in strong windsas both these conditions can be deemed a health and safety risk. | Dependant onweather | Dependant onweather | Dependant onweather | None |
| Last one & Duck and run | Danger of injury from hard surfaces. | The inflatable must never be mounted unless the inflatable bed is fully inflated whether the inflatable is in operation or not as this can lead to serious injury. | 1 | 4 | 4 | None |
| Last one & Duck and run | Injury through lack ofsupervision. | A fully trained operator must be present with the equipment at all times, in the event that theoperator is not in view. Do Not enter the any circumstances. | 1 | 5 | 5 | None |
| Last one & Duck and run | Tripping over anchorage points,spare equipment, electrical cables | Anchor points used as per manufacturer’s instructions and spare equipment erectedsafely or stowed away. Where possible electrical cable does not cross any public pathway. | 1 | 1 | 1 | In the event of large numbers of participants attending or largeevents, additional safety fencing is erected, electrical cables will be erected overhead or covered and |
| Last one & Duck and run | Injury through incorrectpositioning. | Do not move or try to reposition the inflatable under any circumstances and ensurethat the anchors are in place at all times. | 1 | 2 | 2 | None |
| Last one & Duck and run | Petrol Blower, GeneratorRisk of fire | Blowers/generators filled with fuel before delivery, units are fire retardant. | 3 | 1 | 1 | All spare fuel is stored in suitable marked container, and in a safelocation, units switched off during re fuelling, |
| Last one & Duck and run | Choking | No food drinks or chewing gum to be allowed on or near the Inflatable. | 1 | 4 | 4 | None |
| Last one & Duck and run | Injury through 3rd party items | All shoes, glasses, jewellery, badges MUST be removed before using this Inflatable. | 1 | 5 | 5 | None |
| Last one & Duck and run | Danger of fire. | No smoking or barbecues near the Inflatable at any time. | 1 | 5 | 5 | None |
| Last one & Duck and run | Last one arm | 8 players at a time arm is inflatable so you have to jump over the arm . no grabbing the arm or trying to run around the inflatable. | 1 | 3 | 3 | None |
| Last one & Duck and run | Injury through 3rd party &spectators. | Always ensure that the area surrounding the Inflatable is not overcrowded. | 2 | 3 | 6 | None |
| Last one & Duck and run | Emergency | In the event that someone is seriously injured, DO NOT move the individual, leave the inflatable switched on and dial 999 immediately. | N/a | N/a | N/a | N/a |
| Last one & Duck and run | Injury from bunting | bunting should be supervised to ensure participants do not become tangled.Supervisor should be provided at all time. | 1 | 2 | 2 | None |
| Last one & Duck and run | Injury through lack of inflatablepressure or suffocation. | Do not allow anyone to be on the Inflatable during inflation or deflation as this can beEXTREMELY DANGEROUS. | 1 | 2 | 2 | None |
| Last one & Duck and run | Injury through insecureanchorage. | Never use this unit without proper anchorage in place, It may be blown over in certainwind conditions, If the inflatable unit is not anchored correctly please ensure you tell the erection team before they leave as we keep a tight schedule and may not be ableto return immediately. | 1 | 5 | 5 | None |

L=Likelihood S=Severity L\*S= Risk 1=Low 5=High

Risk is worked out using numbers 1 - 5. The likelihood is given a number and this is multiplied by the number given to the severity of the risk.

The result = the risk factor. This generic risk assessment is brief and we have our own individual assessments for each individual risk, 25 being the worst possible outcome, any item reaching 25 would give serious cause for concern & we would not be able to erect the unit. It is recommended that clients undertake their own risk assessment to suit their requirements.